Missing resource files; asterisk means it is missing from P4W.

**DRAIN:**

number

description

location

use map coordinates

-xy\_coordinate\_system

\*\*\* -z\_coordinate\_system

width

hydraulic conductivity

thickness

Z

**GRID:**

\*\*\*Grid origin (add to screen, new tab?)

\*\*\*Grid angle (add to screen)

**LEAKY\_BC:**

\*\*\*thickness description should be BC\_LEAKY\_HYD\_COND.rtf.

\*\*\*Hydraulic conductivity description should be BC\_LEAKY\_THICKNESS.rtf.

\*\*\*-elevation*property*

\*\*\*-z\_coordinate\_system

**MEDIA:**

-shell + x,y,z

-tortuosity

**PRINT\_FREQUENCY:**

-end\_of\_period\_default

-restart\_file

-zone\_flow (txt) (out of alphabetical order)

\*\*\*-zone\_flow\_heads (xyzt)

-zone\_flow\_tsv

**PRINT\_INITIAL:**

-HDF\_media\_properties

\*\*\*When you click on a check box, it should probably display the appropriate file description.

\*\*\*PRINT\_LOCATIONS:

omit?

RIVER:

use map coordinates (-xy\_coordinate\_system **(**grid **|** map**))**

\*\*\*bottom, (use map coordinates), -z\_coordinate\_system **(**grid **|** map**)**

**SPECIFIED\_HEAD:**

exterior cells only

**STEADY\_FLOW:**

growth factor

**TIME\_CONTROL:**

-time\_start

\*\*\*TITLE:

omit?

WELL:

\*\*\*When bottom elevation, top elevation get focus in grid, should display -elevation description

\*\*\*Same when Depth if selected, should show -depth.

use map coordinates (-xy\_coordinate\_system)

use map coordinates (-z\_coordinate\_system)

ToDo:

Switch Elevation and Depth buttons?

With Depth, LSD and Use Map coordinates are disabled.

With Elevation, LSD and Use Map coordinates are enabled.

Move Use Map coordinates on line with LSD.

ZONE\_FLOW:

Number

Description

Combination?

\*\*\*-write\_heads\_xyzt